NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/302 Floor channels

NBS Specification:



This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-Drainage-ChannelsKSBC150BoxChannel)

* [310 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-Drainage-ChannelsKSBC150BoxChannel)

Product Specification:

KVBC150 Box Channel

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Vinyl Box Channel

 • Type: KVBC150 / KVSBC200 / KVBC300

 • Length:

 • Loading class to BS EN 1433: A15 /B125 /C250 /D400

 • Fall: Fall 150’ to ‘Fall 1:150 (0.67%) /Fall 1:50 (2%) /Fall 1:100 (1%)

 • Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

 • Channel profile: Box section reinforcement /Double box section reinforcement /Round bottom /Safety edge /Solid bar reinforcement /Standard /'V' bottom

 • Flange: Flange connection at channel joint and neoprene gasket /Flange flush with channel joint

 • Gully: Central Gully KV285/165 /End Gully KV285/165

 • Grating:

Suggested Specification:

KVBC150 Box Channel

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Vinyl Box Channel

 • Type: KVBC200

 • Length: 3000mm

 • Loading class to BS EN 1433: B125

 • Fall: Fall 1:150 (0.67%)

 • Material: 1.4301 (304) stainless steel

 • Channel profile: Standard

 • Flange: Flange connection at channel joint and neoprene gasket

 • Gully: Central Gully KV285/165

 • Grating: Kent Ladder Grating KMG150