NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:



This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVCR2654RD)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVCR2654RD)

Product Specification:

KVCR265/4”RD

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Gully

 • Type: KVCR265/4” RD /KVCR365/6” RD /KVCR265/4” SQ /KVCR365/6” SQ

 • Height: Manufacturer's standard /Bespoke

 • Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

 • Flange type: 4” 150lb R/F S/O ANSI Flange /4” PN10 R/F S/O Flange /Damp proof membrane flange /Holding flange /Puddle flange

 • Side inlets:

 - Type: 1½” BSP nipple /1½” BSP socket /50 mm push fit /Above ground funnel

 - Angle: 45° /90° /Bespoke

 • Cover/ Grating: Perforated grating /Sealed /Slotted

 • Filter basket: Not required /Required /Required, with chain /Required, with separate filter basket

 • Accessories: None /Heavy duty suction cup /Hinged self-sealing stainless bung

Suggested Specification:

KVCR265/4”RD

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Gully

 • Type: KVCR265/4” RD

 • Height: Manufacturer's standard

 • Material: 1.4401 (316) stainless steel

 • Flange type: Holding flange

 • Cover/ Grating: Sealed

 • Filter basket: Not required

 • Accessories: Heavy duty suction cup