NBS Specification:



This product is associated with the following NBS Create clause:

45-25-15/313 Stainless steel bollards

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentInternalBollards)

* [170 PROPRIETARY](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentInternalBollards)

Product Specification:

Kent Internal Bollards

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Internal Bollard (KIB101)

• Top: Dome /Flat /Sloped

• Material:

- Type: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

- Finish: 320 grit polished and electropolished /Bead blasted /Bead blasted and electropolished /Electropolished /Satin, 320 grit polished /Powder coated

• Fixing: Buried flange /Cast-in /Flange /Hidden flange

• Cowl: Required /Not required