NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/302 Floor channels

NBS Specification:



This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [310 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

Top Slot Channel

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Slot Channel

 • Type: KTS125/200/100-10 /KTS125/250/100-10 /KTS125/300/100-10 /KTS175/250/100-10 /KTS175/300/100-10 /KTS175/350/100-10

 • Material: Grade 1.4307 (304L) stainless steel /Grade 1.4404 (316L) stainless steel

 • Loading: BS EN 124 B125 /BS EN 124 C250 /BS EN 124 D400

 • Channel slot:

 - Throat: Curved /Hidden /Visible

 - Type: Slot channel /Top slot channel

 • Connectors: Channel connector /Drop connector /Silt trap connector

 • End cap: Slot channel end cap

 • Access cover: Recessed access box /Recessed access box with side fixed visible slot /Recessed access box with centre fixed visible slot

 • Outlet point: Bottom /Side /End

Suggested Specification:

Top Slot Channel

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Slot Channel

 • Type: KTS125/200/100-10

 • Material: Grade 1.4404 (316L) stainless steel

 • Loading: BS EN 124 B125

 • Channel slot:

 - Throat: Visible

 - Type: Slot channel

 • Connectors: Channel connector

 • End cap: Slot channel end cap

 • Access cover: Recessed access box

 • Outlet point: Bottom