NBS Specification:



This product is associated with the following NBS Create clause:

45-75-95/465 Wall protection panels

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N10 General fixtures/ furnishings/ equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentWallGuards)

* [350 MISCELLANEOUS FITTINGS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentWallGuards)

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/products/unframed-isolated-trims-skirtings-sundry-items/P20.aspx)

* [170 PROPRIETARY](https://www.ribaproductselector.com/products/proprietary/P20_170.aspx)

Product Specification:

Kent Cleanroom Crash Rail

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

USA Local: 781 374 8377

Tel: +353 53 914 3216

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Cleanroom Crash Rail

• Type: KCRCR102-6-76 / KCRCR76-6-76 / KCRCR152-6-76

• Length: 12ft. /Bespoke

• Material:

- Type: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

- Finish: No. 4 Finish (240 grit polished)

Suggested Specification:

Kent Cleanroom Crash Rail

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

USA Local: 781 374 8377

Tel: +353 53 914 3216

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Cleanroom Crash Rail

• Type: KCRCR102-6-76

• Length: 12ft.

• Material:

- Type: 1.4301 (304) stainless steel

- Finish: No. 4 Finish (240 grit polished)